The Data Type in this certificate must be interpreted as:

**As Found**

Calibration data collected before the unit is adjusted and / or repaired.

**As Left**

Calibration data collected after the unit has been adjusted and / or repaired.

**Found-Left**

Calibration data collected without any adjustment and / or repaired performed.

This Certificate may contain data that is not covered by the Scope of Accreditation. Unaccredited material, where applicable is indicated by an asterisk (\*), or confined to clearly marked sections. Functional (Pass/Fail) tests are not accredited.

Mu Li

CALIBRATION\_ENGINEER\_TITLE QC\_APPROVAL\_TITLE